{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["2021工业废气","2021有机废气 (2)","2021锅炉废气噪声","2021废水","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"2021工业废气","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"merged":[[0,0,0,4],[2,0,28,0],[2,1,5,1],[2,3,5,3],[2,4,5,4],[2,5,51,5],[2,6,51,6],[6,1,9,1],[6,3,9,3],[6,4,9,4],[10,1,13,1],[10,3,13,3],[10,4,13,4],[14,1,17,1],[14,3,17,3],[14,4,17,4],[18,1,21,1],[18,3,21,3],[18,4,21,4],[22,1,25,1],[22,3,25,3],[22,4,25,4],[29,0,30,0],[29,1,30,1],[29,3,30,3],[29,4,30,4],[31,1,34,1],[31,3,34,3],[31,4,34,4],[37,0,38,0],[37,1,38,1],[37,3,38,3],[37,4,38,4],[39,0,40,0],[39,1,40,1],[39,3,40,3],[39,4,40,4],[42,0,43,0],[42,1,43,1],[42,3,43,3],[42,4,43,4],[44,0,45,0],[44,1,45,1],[44,3,45,3],[44,4,45,4],[46,0,47,0],[46,1,47,1],[46,3,47,3],[46,4,47,4],[48,0,49,0],[48,1,49,1],[48,3,49,3],[48,4,49,4],[50,0,51,0],[50,1,51,1],[50,3,51,3],[50,4,51,4]],"flags":["formulas_cached_only"]}
["2021廢氣、噪聲、工業粉塵、食堂煙火監測項目清單"]
["名稱","採樣點","監測顯目","監測頻率","執行標準","確認","二次確認"]
["工業廢氣廢氣監測","DA01  1#酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5","党建国"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA02 2# 酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA03 3#酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA04 4#酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA05 5#酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA06 6#酸性廢氣處理排放口","NOX","1次/半年","《電鍍污染物排放標準》（GB21900-2008）中的表5"]
[null,null,"HCL"]
[null,null,"氟化物"]
[null,null,"硫酸霧"]
[null,"DA07 2#号粉尘排放口","颗粒物","1次/半年"]
[null,"DA08 1#号粉尘排放口","颗粒物","1次/半年"]
[null,"DA093 9#号粉尘排放口","颗粒物","1次/半年"]
["有機氣體監測","DA0103号有機廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
[null,"DA011 7#酸性廢氣處理排放口","NOX","1次/半年"]
[null,null,"HCL"]
[null,null,"SO2"]
[null,null,"硫酸霧"]
["碱性废气监测","DA012  1号碱性废气排放口","碱雾、氨（氨气）","1次/半年","恶臭污染物排放标准GB 14554-93"]
["碱性废气监测","DA013  2号碱性废气排放口","碱雾、氨（氨气）",null,"恶臭污染物排放标准GB 14554-93"]
["有機氣體監測","DA14  5号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA15  1号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["碱性废气监测","DA016  3号碱性废气排放口","碱雾 "]
["有機氣體監測","DA17  2号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA18  4号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["有機氣體監測"," 厂界 1号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["有機氣體監測"," 厂界  2号有机廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
["食堂煙火監測","食堂煙火處理後排放口","煙塵","1次/半年","GB18483-2001"]
[null,null,"黑度"]

{"sheet":"2021有机废气 (2)","index":1,"n_rows":38,"n_cols":7,"rows_kept":38,"merged":[[0,0,0,4],[2,0,5,0],[2,1,3,1],[2,3,3,3],[2,4,37,4],[2,5,37,5],[2,6,37,6],[4,1,5,1],[4,3,5,3],[6,0,9,0],[6,1,7,1],[6,3,7,3],[8,1,9,1],[8,3,9,3],[10,0,13,0],[10,1,11,1],[10,3,11,3],[12,1,13,1],[12,3,13,3],[14,0,17,0],[14,1,15,1],[14,3,15,3],[16,1,17,1],[16,3,17,3],[18,0,21,0],[18,1,19,1],[18,3,19,3],[20,1,21,1],[20,3,21,3],[22,0,25,0],[22,1,23,1],[22,3,23,3],[24,1,25,1],[24,3,25,3],[26,0,29,0],[26,1,27,1],[26,3,27,3],[28,1,29,1],[28,3,29,3],[30,0,33,0],[30,1,31,1],[30,3,31,3],[32,1,33,1],[32,3,33,3],[34,0,35,0],[34,1,35,1],[34,3,35,3],[36,0,37,0],[36,1,37,1],[36,3,37,3]],"flags":["formulas_cached_only"]}
["2021有机废气監測項目清單"]
["名稱","採樣點","監測顯目","監測頻率","執行標準","確認","二次確認"]
["有機氣體監測","DA010  3号有機廢氣排放口","苯 ","1次/半年","印刷性行业挥发性有机化合物排放标准DB44/815-2010"]
[null,null,"挥发性有机物"]
[null,"DA010  3号有機廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA14  5号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"DA14  5号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA15  1号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"DA15  1号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA17  2号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"DA17  2号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","DA18  4号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"DA18  4号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","      6号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"      6号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","      7号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"      7号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測","      8号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
[null,"      8号有机廢氣进气口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測"," 厂界 1号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]
["有機氣體監測"," 厂界  2号有机廢氣排放口","苯 ","1次/半年"]
[null,null,"挥发性有机物"]

{"sheet":"2021锅炉废气噪声","index":2,"n_rows":20,"n_cols":7,"rows_kept":20,"merged":[[0,0,0,4],[2,0,5,0],[2,1,5,1],[2,3,5,3],[2,4,5,4],[2,5,10,5],[2,6,10,6],[6,0,9,0],[6,3,9,3],[6,4,10,4]],"flags":["formulas_cached_only"]}
["2021锅炉廢氣、噪聲 監測項目清單"]
["名稱","採樣點","監測顯目","監測頻率","執行標準","確認","二次確認"]
["鍋爐廢氣監測","鍋爐廢氣處理後排放口","NOX","1次/半年","（鍋爐大氣污染物最高允許排放限值DB44/765-2019","党建国"]
[null,null,"SO2"]
[null,null,"颗粒物"]
[null,null,"格林曼黑度"]
["廠界噪聲監測","1＃廠界西外1米","噪聲","1次/半年","GB12348-2008）三類"]
[null,"2＃廠界北外米","噪聲"]
[null,"3＃廠界東外3米","噪聲"]
[null,"4＃廠界南外1米","噪聲"]
[]
[]
[null,"  2＃"," "]
[null,null,"       北"]
[null,"         1＃                              3＃"]
[]
[]
[null,"                        4＃"]
[null,"                     萬安路"]
[null,"                                                   西環路"]

{"sheet":"2021废水","index":3,"n_rows":72,"n_cols":7,"rows_kept":72,"merged":[[0,0,0,6],[2,0,11,0],[2,1,11,1],[2,3,11,3],[2,4,11,4],[2,5,71,5],[2,6,11,6],[12,0,31,0],[12,1,31,1],[12,3,31,3],[12,4,31,4],[12,6,31,6],[32,0,51,0],[32,1,51,1],[32,3,51,3],[32,4,51,4],[32,6,51,6],[52,0,71,0],[52,1,71,1],[52,3,71,3],[52,4,71,4],[52,6,71,6]],"flags":["formulas_cached_only"]}
["2021廢水監測項目清單"]
["名稱","採樣點","監測顯目","監測頻率","執行標準","確認","二次確認"]
["廢水總排口 ","總排放口","PH","2021年2-12月共計11次，每月1次","电镀水污染物排放标准DB 44/1597-2015,/","党建国"]
[null,null,"COD"]
[null,null,"總銅"]
[null,null,"總鎳"]
[null,null,"總磷"]
[null,null,"總氰化物"]
[null,null,"氨氮"]
[null,null,"總氮"]
[null,null,"氟化物"]
[null,null," "]
["廢水總排口20項全項檢測",null,"PH","2021年1月份","电镀水污染物排放标准DB 44/1597-2015,/"]
[null,null,"COD"]
[null,null,"總銅"]
[null,null,"總鎳"]
[null,null,"總磷"]
[null,null,"總氰化物"]
[null,null,"氨氮"]
[null,null,"懸浮物"]
[null,null,"總鉻"]
[null,null,"六價鉻"]
[null,null,"總鎘"]
[null,null,"總銀"]
[null,null,"總鉛"]
[null,null,"總汞 "]
[null,null,"總鋅"]
[null,null,"總鐵"]
[null,null,"總鋁"]
[null,null,"總氮"]
[null,null,"石油類"]
[null,null,"氟化物"]
["綜合廢水20項全項檢測",null,"PH","2021年次/季度","电镀水污染物排放标准DB 44/1597-2015,/"]
[null,null,"COD"]
[null,null,"總銅"]
[null,null,"總鎳"]
[null,null,"總磷"]
[null,null,"總氰化物"]
[null,null,"氨氮"]
[null,null,"懸浮物"]
[null,null,"總鉻"]
[null,null,"六價鉻"]
[null,null,"總鎘"]
[null,null,"總銀"]
[null,null,"總鉛"]
[null,null,"總汞 "]
[null,null,"總鋅"]
[null,null,"總鐵"]
[null,null,"總鋁"]
[null,null,"總氮"]
[null,null,"石油類"]
[null,null,"氟化物"]
["絡合廢水20項全項檢測",null,"PH","2021年次/季度","电镀水污染物排放标准DB 44/1597-2015,/"]
[null,null,"COD"]
[null,null,"總銅"]
[null,null,"總鎳"]
[null,null,"總磷"]
[null,null,"總氰化物"]
[null,null,"氨氮"]
[null,null,"懸浮物"]
[null,null,"總鉻"]
[null,null,"六價鉻"]
[null,null,"總鎘"]
[null,null,"總銀"]
[null,null,"總鉛"]
[null,null,"總汞 "]
[null,null,"總鋅"]
[null,null,"總鐵"]
[null,null,"總鋁"]
[null,null,"總氮"]
[null,null,"石油類"]
[null,null,"氟化物"]

{"sheet":"Sheet2","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}